**INTEGRATED GREEN SOLUTIONS**Neo-Metro draws from the experience of its parent company, Acorn Engineering Company, a renowned producer of stainless steel plumbing fixtures, to sculpt luxury bath furnishings out of 80%recycled stainless steel. With its durable functionality and contemporary look, stainless steel outlasts other materials and never goes out of style.

Picture a hotel or restaurant bathroom with a custom basin, manufactured from recycled material such as stainless steel, and discreetly fitted with a tankless water heater and the most efficient water-saving engineering possible. Add in a low-flow or dual flush toilet in addition to a waterless or pint-flow urinal. All of these water and energy saving fixtures are possible from Neo-Metro, complete with a variety of finishes and powder-coated colors to choose from and customize. Because we research, design and manufacture our own products in North America, customers have the benefit of going to one supplier to get the job done. Further, a majority of Neo-Metro products earn LEED points for new buildings and offer significant reductions in cost and energy use for new or existing properties. In this way, Neo-Metro supports a "whole building" approach to commercial sustainability by offering integrated products and solutions to a green building's many challenges.

**SUSTAINABLE COMMERCIAL PLUMBING SOLUTIONS FOR RESIDENTIAL & HOSPITALITY APPLICATIONS**Neo-Metro's series of water-saving and energy-conscious products give specifiers and architects the flexibility to maximize green opportunities in plumbing:

\*All fixtures are made from 80% recycled stainless steel.

|  |  |
| --- | --- |
| **System M2 multiple-station wash basins & HWS all-inclusive circular fountains** | * One plumbing connection for multiple basins
* Can be outfitted with sensor-activated fixtures
* Compatible with Chronomite tankless water heater
 |
| **High Efficiency and Cistern Style Dual Flush toilets, including MiniLoo, Euro-Urban Contour, Metaal wall-mounted models** | * High efficiency model: low-flow (1.28gpf) flush
* 1.2 gallon Cistern Style model available
* 0.5 gallons per flush with AcornVac vacuum plumbing
 |
| **Waterless Urinal** | * Proven technology - No water necessary
* No need for harmful chemical cartridges
 |
| **High Efficiency Urinals** | * Available in 0.125gpf model
* 0.5 gpf with AcornVac vacuum plumbing
 |
| **Chronomite Tankless Electric Water Heater** | * 98% energy efficient
* Conserves water
* Lower maintenance and operational costs
* Maintains health and security
 |

**CUSTOMER BENEFITS**

* Recycled stainless steel
* Lower maintenance & operational costs
* Saves water
* Saves installation time
* One manufacturer
* ADA compliant products
* Customizable
* Sterile material

**SYSTEM M2 BASIN LINE**Neo-Metro's System M2 multiple-station wash basins offer a highly-customizable platform for the optimal level of function, sustainability and water savings. Units require only one plumbing connection to provide hand washing stations in multiple basin configurations or wash stations. The result: lower installation and maintenance costs. Basins are optionally outfitted with push button metering valves, sensor-activated fixtures and a tankless water heater for quick, easy hand washing with minimal water use. Made from a recycled stainless steel material base, units provide years of trouble-free service with an engineered and manufactured valve design that has been in use for over 50 years.

**WATER SAVING TOILETS**Neo-Metro's stainless steel toilets have an industrialized modern appeal. With their clean, utilitarian form and strength, 80%recycled stainless steel fixtures will outlast other fixtures and never go out of style.

Neo-Metro toilets are compatible with a variety of water-saving flush valves, no special tools or adaptation required. A 1.28-gpf High Efficiency Toilet from Neo-Metro is easily integrated into a building's plans for water conservation. Additionally, many feature an In-Wall Cistern Style System, which minimizes water savings by allowing users to select either 1.6 or 0.8-gallons, for an average of 1.2 gallons per flush. The MiniLoo, Euro-Urban Contour, and Metaal toilets from Neo-Metro all feature this dual flush system. In addition, all contribute to a building's overall water use reduction and can earn LEED points in sections WE C3.1 and C3.2 for 20-30%savings.

**WATER SAVING URINALS
 Waterless Urinal**Neo Metro's Waterless Urinal works efficiently with absolutely no water required, furthering Neo-Metro's commitment to the environment. There is no need for expensive replacement liquid cartridges and therefore, no chemicals are dumped into any landfills. The durable stainless steel product is wall mounted and can be installed to meet ADA requirements. Units also come in satin or high-polish finish, and an Enviro-Glaze powder coating can be color-matched to a variety of sophisticated hues. And like so many other green offerings from Acorn, this system is third-party certified as eco-friendly, earning LEED points for water savings which work towards achieving US Green Building certification.

 **High Efficient Urinal**The new High Efficiency Urinal is similar in design to the waterless urinal, with its sleek industrial-chic simplicity. Featuring a low-flow flush valve, this unit utilizes a 0.125 Pint Flow rate and also works efficiently with AcornVac's half-gallon flush.